Engineering Excellence

# Specifications & Materials

Precision-engineered tubular carcasses, premium baskets, high-grade shutters, and world-class hardware — defining the Adeetya’s standard.

## Tubular Carcass Types

#### Powder Coated Carcass

Raw Material: Cold Rolled Cold Annealed (CRCA) Steel Pipe 19mm x 19mm x 19swg
Finish: Black / Silver Powder coated with seven tank process, Thickness-50 microns

#### Stainless Steel 304 Carcass

Raw Material: St. Steel AISI 304 Grade, 19mm x 19mm x 19swg
Finish: Electro Polished or Buff

#### Stainless Steel 202 Carcass

Raw Material: St. Steel AISI 202 Grade, 19mm x 19mm x 19swg
Finish: Electro Polished or Buff

## Basket Types

#### Powder Coated Basket

Raw Material: CRCA, Dia.10mm x 19swg
Basket Base: M.S; Dia.3mm
Support Bar: M.S; Dia.5mm
Finish: Black/Silver Powder coated, seven tank process, 50 microns

#### Stainless Steel 304 Basket

Raw Material: St. Steel AISI 304 Grade, Dia.10mm x 19swg
Basket Base: St. Steel AISI 304 Grade; Dia.3mm
Support Bar: St. Steel AISI 304 Grade Dia.5mm
Finish: Electro Polished or Buff

#### Stainless Steel 202 Basket

Raw Material: St. Steel AISI 202 Grade, Dia.10mm x 19swg
Basket Base: St. Steel AISI 202 Grade; Dia.3mm
Support Bar: St. Steel AISI 202 Grade Dia.5mm
Finish: Electro Polished or Buff
Plain laminated base of 3mm thickness available on demand

## Shutters & Carcass Materials

#### Shutters (Four side edge banded)

• Laminated Shutters in MDF / Ply / Block board
• Acrylic High Gloss Shutters in MDF / Ply (German Imported Raw Material)
• Ultra Violet High Gloss Shutters in MDF
• PU High Gloss Shutters in MDF – Merino
Board below Granite: Eco Link Tetra Pack Board or Marine Ply Thickness 12mm

#### Wall Cabinets, Tall Units, Wardrobe & Loft Cover

• Particle Board both side laminated (BSL) 18mm Thickness
• Marine Ply both side laminated (BSL) on 16mm board
• BWR Marine Ply both side laminated (BSL) on 16mm board
• Calibrated Ply both side laminated (BSL) on 18mm board

## Hardware & Fittings

#### Channels

Bottom Mounted Drawer Slide or Telescopic Channel - Hettich / Moda
Quadra or Innotech Channel with/without silent - Hettich
Tandom Boxes Slides - Adeetyas / Hettich / Haffle / Grass with Silent System

#### Hinges & Lift Ups

Hinges: Auto Closing, Silent - Hettich / Moda / Haffle
Lift Ups: Hettich / Moda / Haffle
Handle: Black Powder Coated, Aluminium Casted Chrome Plated, Aluminium Profile

#### Other Hardware

Caster Wheel: Ball Bearing Dia.25mm Teflon Coated
Hardware: Metric Threads, M.S. - Zink/Nickel Plated or Blackodised
Work Top: Granite top / Synthetic top / Post form laminated top / As per choice

## Warranty

#### Lifetime Anti-Weather Warranty

12 Years against rust on Stainless Steel 304 Grade accessories and frame

#### Lifetime Warranty on Fittings

8 Years against manufacturing defects (with normal usage)

#### Particle Board Carcass

3 Years warranty against manufacturing defects

#### MDF / Acrylic / UV Doors

3 Years warranty against manufacturing defects

#### Marine Ply Carcass & Doors

1 Year warranty against manufacturing defects

*Conditions apply. Warranty valid under normal usage and proper maintenance.

All specifications are customizable as per your requirements. Contact our design team for personalized solutions.

Tailor-made kitchens Factory-finished furniture Pan-India installation